<?xml version="1.0" encoding="utf-8"?>
<TcPlcObject Version="1.1.0.1" ProductVersion="3.1.4024.12">
  <DUT Name="ST_SunspecNameplateRatings" Id="{d43d4b8b-dd50-4ed8-ac51-53563f3eb7b3}">
    <Declaration><![CDATA[// Sunspec register 40.122 - 40.149 (Size 28)
TYPE ST_SunspecNameplateRatings :
STRUCT
	// Model value
	uiID : UINT;
	
	// Model length
	uiL : UINT;
	
	// Type of DER device
	wDERTyp : WORD;
	
	// Continuous power output capability of the inverter
	uiWRtg : UINT;
	
	// Continuous power output capability of the inverter scaling factor
	uiWRtgSF : INT;
	
	// Continuous volt-ampere output capability of the inverter
	uiVARtg : UINT;
	
	// Continuous volt-ampere output capability of the inverter scaling factor
	uiVARtgSF : INT;
	
	// Continuous VAR capability of the inverter in quadrant 1
	iVArRtgQ1 : INT;
	
	// Continuous VAR capability of the inverter in quadrant 2
	iVArRtgQ2 : INT;
	
	// Continuous VAR capability of the inverter in quadrant 3
	iVArRtgQ3 : INT;
	
	// Continuous VAR capability of the inverter in quadrant 4
	iVArRtgQ4 : INT;
	
	// Continuous VAR capability of the inverter in quadrant 1-4 scaling factor
	iVArRtgSF : INT;
	
	// Maximum RMS AC current level capability of the inverter
	uiARtg : UINT;
	
	// Maximum RMS AC current level capability of the inverter scaling factor
	uiARtgSF : INT;
	
	// Minimum power factor capability of the inverter in quadrant 1
	iPFRtgQ1 : INT;
	
	// Minimum power factor capability of the inverter in quadrant 2
	iPFRtgQ2 : INT;
	
	// Minimum power factor capability of the inverter in quadrant 3
	iPFRtgQ3 : INT;
	
	// Minimum power factor capability of the inverter in quadrant 4
	iPFRtgQ4 : INT;
	
	// Minimum power factor capability of the inverter in quadrant 1-4 scaling factor
	iPFRtgSF : INT;
	
	// Nominal energy rating of storage device
	uiWHRtg : UINT;
	
	// Nominal energy rating of storage device scaling factor
	uiWHRtgSF : INT;
	
	// The usable capacity of the battery
	uiAhrRtg : UINT;
	
	// The usable capacity of the battery scaling factor
	uiAhrRtgSF : INT;
	
	// Maximum rate of energy transfer into the storage device
	uiMaxChaRte : UINT;
	
	// Maximum rate of energy transfer into the storage device scaling factor
	uiMaxChaRteSF : INT;
	
	// Maximum rate of energy transfer out of the storage device
	uiMaxDisChaRte : UINT;
	
	// Maximum rate of energy transfer out of the storage device scaling factor
	uiMaxDisChaRteSF : INT;
	
	// Padding register
	wPad : WORD;
	
END_STRUCT
END_TYPE
]]></Declaration>
  </DUT>
</TcPlcObject>