<?xml version="1.0" encoding="utf-8"?>
<TcPlcObject Version="1.1.0.1" ProductVersion="3.1.4026.7">
  <GVL Name="GVL_SCADA" Id="{8186ff04-764f-4b24-8a6b-d0a44d528e6f}">
    <Declaration><![CDATA[{attribute 'qualified_only'}
VAR_GLOBAL
	stHMIInterface : ARRAY [0..1] OF ST_STRING_HMI_INTERFACE;
	
	stAckAlarmsButton : ST_HMI_CONTROL_BUTTON := (xRelease := TRUE);
	
	// Butotn to switch all components into manual mode
	stAllToManualModeButton : ST_HMI_CONTROL_BUTTON;
	
	// Button to switch all components in to automatic mode
	stAllToAutoModeButton : ST_HMI_CONTROL_BUTTON;
	
	stAutomaticModeHMI : ST_AUTO_HMI_INTERFACE;
	
	// Requested control mode by HMI
	eRequestedControlMode : E_BMS_CONTROL_MODE;
	
	// Current control mode
	eCurrentControlMode : E_BMS_CONTROL_MODE;
	
	// Can change current control mode
	xCanChangeControlMode : BOOL;
	
	// Current battery power
	diCurrentBatteryPower : DINT;
	
	xDummy : BOOL := FALSE;
END_VAR]]></Declaration>
  </GVL>
</TcPlcObject>