<?xml version="1.0" encoding="utf-8"?>
<SafetyDeviceDesc Crc="3021705149" FileFormatVersion="1.8">
  <AliasDeviceType>
    <Type>4</Type>
    <SubType>290</SubType>
    <VendorId>2</VendorId>
  </AliasDeviceType>
  <SDSID>3</SDSID>
  <SafetyAliasDevice>
    <ObjectId>50921473</ObjectId>
    <LinkingMode>Automatic</LinkingMode>
    <ConnectionId>3</ConnectionId>
    <ConnectionMode>master</ConnectionMode>
    <ConnectionType>FSoE</ConnectionType>
    <MapDiag>false</MapDiag>
    <MapInputs>false</MapInputs>
    <MapOutputs>false</MapOutputs>
    <MapState>false</MapState>
    <ModuleFaultIsComErr>false</ModuleFaultIsComErr>
    <SafeAddress>3</SafeAddress>
    <Watchdog>100</Watchdog>
    <ComErrAck Type="Unset" />
    <Params>
      <Param Index="4320" SubIndex="1">0000</Param>
      <Param Index="4320" SubIndex="2">0000</Param>
      <Param Index="32768" SubIndex="1">00</Param>
      <Param Index="32768" SubIndex="2">01</Param>
      <Param Index="32768" SubIndex="3">01</Param>
      <Param Index="32768" SubIndex="4">00</Param>
      <Messages>
        <IO>
          <Name>FSoE Master CMD</Name>
          <Index>28672</Index>
          <SubIndex>1</SubIndex>
          <DataType>USINT</DataType>
          <Direction>Out</Direction>
          <SafetyType>ProtocolData</SafetyType>
          <BitSize>8</BitSize>
          <BitOffsMessage>0</BitOffsMessage>
          <BitOffsData>-1</BitOffsData>
        </IO>
        <IO>
          <Name>OutputChannel1</Name>
          <Index>28673</Index>
          <SubIndex>1</SubIndex>
          <DataType>BIT</DataType>
          <Direction>Out</Direction>
          <SafetyType>SafetySil3</SafetyType>
          <BitSize>1</BitSize>
          <BitOffsMessage>8</BitOffsMessage>
          <BitOffsData>0</BitOffsData>
        </IO>
        <IO>
          <Name>OutputChannel2</Name>
          <Index>28673</Index>
          <SubIndex>2</SubIndex>
          <DataType>BIT</DataType>
          <Direction>Out</Direction>
          <SafetyType>SafetySil3</SafetyType>
          <BitSize>1</BitSize>
          <BitOffsMessage>9</BitOffsMessage>
          <BitOffsData>1</BitOffsData>
        </IO>
        <IO>
          <Name>OutputChannel3</Name>
          <Index>28673</Index>
          <SubIndex>3</SubIndex>
          <DataType>BIT</DataType>
          <Direction>Out</Direction>
          <SafetyType>SafetySil3</SafetyType>
          <BitSize>1</BitSize>
          <BitOffsMessage>10</BitOffsMessage>
          <BitOffsData>2</BitOffsData>
        </IO>
        <IO>
          <Name>OutputChannel4</Name>
          <Index>28673</Index>
          <SubIndex>4</SubIndex>
          <DataType>BIT</DataType>
          <Direction>Out</Direction>
          <SafetyType>SafetySil3</SafetyType>
          <BitSize>1</BitSize>
          <BitOffsMessage>11</BitOffsMessage>
          <BitOffsData>3</BitOffsData>
        </IO>
        <IO>
          <Name />
          <Index>0</Index>
          <SubIndex>0</SubIndex>
          <DataType />
          <Direction>Out</Direction>
          <SafetyType>SafetySil3</SafetyType>
          <BitSize>4</BitSize>
          <BitOffsMessage>12</BitOffsMessage>
          <BitOffsData>4</BitOffsData>
        </IO>
        <IO>
          <Name>FSoE Master CRC_0</Name>
          <Index>28672</Index>
          <SubIndex>3</SubIndex>
          <DataType>UINT</DataType>
          <Direction>Out</Direction>
          <SafetyType>ProtocolData</SafetyType>
          <BitSize>16</BitSize>
          <BitOffsMessage>16</BitOffsMessage>
          <BitOffsData>-1</BitOffsData>
        </IO>
        <IO>
          <Name>FSoE Master ConnID</Name>
          <Index>28672</Index>
          <SubIndex>2</SubIndex>
          <DataType>UINT</DataType>
          <Direction>Out</Direction>
          <SafetyType>ProtocolData</SafetyType>
          <BitSize>16</BitSize>
          <BitOffsMessage>32</BitOffsMessage>
          <BitOffsData>-1</BitOffsData>
        </IO>
        <IO>
          <Name>FSoE Slave CMD</Name>
          <Index>24576</Index>
          <SubIndex>1</SubIndex>
          <DataType>USINT</DataType>
          <Direction>In</Direction>
          <SafetyType>ProtocolData</SafetyType>
          <BitSize>8</BitSize>
          <BitOffsMessage>0</BitOffsMessage>
          <BitOffsData>-1</BitOffsData>
        </IO>
        <IO>
          <Name />
          <Index>0</Index>
          <SubIndex>0</SubIndex>
          <DataType />
          <Direction>In</Direction>
          <SafetyType>SafetySil3</SafetyType>
          <BitSize>8</BitSize>
          <BitOffsMessage>8</BitOffsMessage>
          <BitOffsData>0</BitOffsData>
        </IO>
        <IO>
          <Name>FSoE Slave CRC_0</Name>
          <Index>24576</Index>
          <SubIndex>3</SubIndex>
          <DataType>UINT</DataType>
          <Direction>In</Direction>
          <SafetyType>ProtocolData</SafetyType>
          <BitSize>16</BitSize>
          <BitOffsMessage>16</BitOffsMessage>
          <BitOffsData>-1</BitOffsData>
        </IO>
        <IO>
          <Name>FSoE Slave ConnID</Name>
          <Index>24576</Index>
          <SubIndex>2</SubIndex>
          <DataType>UINT</DataType>
          <Direction>In</Direction>
          <SafetyType>ProtocolData</SafetyType>
          <BitSize>16</BitSize>
          <BitOffsMessage>32</BitOffsMessage>
          <BitOffsData>-1</BitOffsData>
        </IO>
      </Messages>
    </Params>
  </SafetyAliasDevice>
</SafetyDeviceDesc>